**Midistomp Six Parts List:**

x1 Printed Circuit Board

(purchase from midistomp.com)

x1 Aluminium Enclosure

<https://bit.ly/35fJvGp> (Black)

<https://bit.ly/2LQ1WKf> (White)

<https://bit.ly/38BrPHl> (Bare Metal)

x5 3PDT Footswitch with bi-color LED ring (red/green or purple/green)

<https://bit.ly/2rK6on1>

x1 SPST Momentary Footswitch

<https://bit.ly/2PHnSs2>

x1 5mm LED bezel

<https://bit.ly/2LSnbLA> (This link is from Australia, but easy to find anywhere)

x1 5mm LED (Red or whatever color you want)

Easy to find anywhere online or locally

x1 USB Panel Mount connector

<https://bit.ly/38v2q26>

x1 SPST momentary button switch

<https://bit.ly/38ARWy3> (easily sourced eslewhere) - must be 10mm or smaller to fit the Midistomp instructions. (with longer wire and different switch placement, it can be bigger smaller etc if desired.

x11 220 Ohm resistors  
Easy to find anywhere online or locally

x1 Teensy 2.0  
<https://bit.ly/2tedVLd>

x1 40-pin header pin strip

<https://bit.ly/34lCbYR>

x16 Lengths of wire 24AWG (x14 50mm, x2 100mm)

Easy to find anywhere – ebay have pre-stripped and pre-soldered wires

x1 USB cable

<https://amzn.to/2qIDsv0>